---
title: Get started · Cloudflare WARP client docs
description: "Before installing and setting up the WARP Client, ensure that your
  device meets the following system requirements:"
lastUpdated: 2025-08-20T21:45:15.000Z
chatbotDeprioritize: false
source_url:
  html: https://developers.cloudflare.com/warp-client/get-started/
  md: https://developers.cloudflare.com/warp-client/get-started/index.md
---

Consumer WARP

This documentation is for the consumer version of WARP. If you are using WARP with Cloudflare Zero Trust, refer to the [Zero Trust documentation](https://developers.cloudflare.com/cloudflare-one/team-and-resources/devices/warp/).

Before installing and setting up the WARP Client, ensure that your device meets the following system requirements:

## Android

| | |
| - | - |
| **OS version** | 5.0+ |

[Download for Android](https://play.google.com/store/apps/details?id=com.cloudflare.onedotonedotonedotone)

## iOS

| | |
| - | - |
| **OS version** | iOS 11+ |

[Download for iOS](https://apps.apple.com/us/app/id1423538627)

## Linux

| | |
| - | - |
| **OS version** | CentOS 8, RHEL 8, Debian 11, Debian 12, Debian 13, Fedora 34, Fedora 35, Ubuntu 20.04, Ubuntu 22.04, Ubuntu 24.04 |
| **Processor** | AMD64 / x86-64 or ARM64 / AArch64 |
| **HD space** | 75 MB |
| **Memory** | 35 MB |
| **Network interface type** | WIFI or LAN |
| **Minimum MTU** | 1360 bytes[1](#user-content-fn-1) |

## Footnotes

1. WireGuard requires 1360 bytes for IPv6 and 1340 bytes for IPv4. MASQUE requires 1350 bytes for IPv6 and 1330 bytes for IPv4. [↩](#user-content-fnref-1)

[Download for Linux](https://pkg.cloudflareclient.com/)

## macOS

| | |
| - | - |
| **OS version** | Big Sur 11.0+, Monterey 12.0+, Ventura 13.0+, Sonoma 14.0+, Sequoia 15.1+ (15.0.x is not supported), Tahoe 26.0+ |
| **Processor** | Intel or M series |
| **HD space** | 75 MB |
| **Memory** | 35 MB |
| **Network interface type** | WIFI or LAN |
| **Minimum MTU** | 1360 bytes[1](#user-content-fn-1) |

## Footnotes

1. WireGuard requires 1360 bytes for IPv6 and 1340 bytes for IPv4. MASQUE requires 1350 bytes for IPv6 and 1330 bytes for IPv4. [↩](#user-content-fnref-1)

[Download for macOS](https://downloads.cloudflareclient.com/v1/download/macos/ga)

## Windows

| | |
| - | - |
| **OS version** | Windows 10, Windows 11, Windows 365 Cloud PC running Windows 11 |
| **Processor** | AMD64 / x86-64 |
| **.NET Framework version** | 4.7.2 or later |
| **HD space** | 184 MB |
| **Memory** | 3 MB |
| **Network interface type** | WIFI or LAN |
| **Minimum MTU** | 1360 bytes[1](#user-content-fn-1) |

## Footnotes

1. WireGuard requires 1360 bytes for IPv6 and 1340 bytes for IPv4. MASQUE requires 1350 bytes for IPv6 and 1330 bytes for IPv4. [↩](#user-content-fnref-1)

[Download for Windows](https://downloads.cloudflareclient.com/v1/download/windows/ga)
